**Combi KOMPACT HW/CW - washbasin and floor-standing WC pan**

Polished satin 304 stainless steel - Wall-mounted - Right hand WC pan

With 2 controls cold water/mixed water

Reference: **161600**

Specification description

Combination unit: washbasin and floor-standing right hand WC pan with recessed toilet roll holder.

Wall-mounted installation with 3 access panels, 2 on the sides and 1 on the top, with theft prevention TORX security screws.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel unit thickness: 2mm.

Rounded corners and edges for improved safety.

Smooth surface for easy cleaning.

Suitable for prisons, police stations, etc.

WC pan is completely welded to washbasin, no screws: makes cleaning easier and prevents concealment of objects.

Washbasin equipped with time flow tap: stainless steel tamperproof push-button and anti-blocking system, 7-second time flow, M½".

Available with 2 buttons cold water/mixed water.

WC equipped with time flow flush valve, 7-second time flow, M¾".

Water inlet: washbasin M½", WC M¾".

Recessed horizontal water outlet: Ø 100mm.

Supplied with washbasin trap.

Easy to install: only one water outlet for both washbasin and WC, water inlet and outlet already connected.

Weight: 36kg.