**SECURITHERM EP pressure-balancing shower mixer**

Wall-mounted single control mixer, sculptured lever

With offset standard connectors

Reference: **2539EPS**

Specification description

Wall-mounted single control mechanical shower mixer.

Ø 40mm ceramic cartridge with pressure-balancing and pre-set maximum temperature limiter.

Anti-scalding safety: HW flow rate is reduced if CW supply fails (and vice versa).

Stable temperature regardless of pressure and flow rate variations in the system.

Flow rate regulated at 9 lpm.

M½" shower outlet with integrated non-return valve.

Mixer with offset standard wall connectors M½" M¾".

Filters and non-return valves.

Mechanical mixer with SECURITHERM pressure-balancing ideal for healthcare facilities, nursing homes, hospitals and clinics.

Shower mixer suitable or people with reduced mobility.

Mixer with 30-year warranty.