**Pressure-balancing mixer with independent control**

EP Mechanical mixer for retractible water taps

Mixer with sculptured lever

Reference: **2542EP**

Specification description

Mechanical mixer only, for deck-mounted independent control.

Single hole mixer with pressure-balancing.

Ø 35mm pressure-balancing ceramic cartridge with pre-set maximum temperature limiter.

Total anti-scalding safety: HW flow rate is reduced if CW supply fails (and vice versa).

Stable temperature regardless of pressure and flow rate variations in the system.

Sculptured control lever.

Chrome-plated brass body.

PEX flexibles F⅜" supplied with filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

Mechanical mixer with SECURITHERM pressure-balancing ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

30-year warranty.