**Straight satin stainless steel grab bar, 1050mm Ø 32mm**

UltraSatin polished satin stainless steel

Ø 32mm

Reference: **50510S**

Specification description

Straight grab bar for people with reduced mobility.

Ø 32 mm tube, 1050mm centres.

Use as grab bar, and support in WCs, showers or baths.

304 bacteriostatic stainless steel.

UltraSatin polished satin stainless steel finish, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to tube by invisible safety bead weld (process exclusive to "ArN-Securit”).

40mm gap between the bar and the wall: minimal space prevents the forearmpassing between the bar and the wall, redusing the risk of fracture in case of loss of balance.

Concealed fixings secured to wall by a 3-hole, 304 stainless steel, Ø 72mm.

304 stainless steel plates and covers.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 135kg.

30-year warranty for grab bar, CE marked.