**Wall-mounted SXS electronic hand washbasin WRAS**

Polished satin 304 stainless steel - Electronic ctrl - W/out upstand

With WRAS approved tap and soap dispenser

Reference: **18431015**

Specification description

Wall-mounted hand washbasin with electronic control.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Without splashback.

Supplied with WRAS approved electronic tap with integrated batteries and solenoid valve, a TMV3 and WRAS approved thermostatic mixing valve and a chrome-plated brass soap or hyrdroalcoholic gel dispenser.

1¼" waste included. Without overflow.

Water savings: flow rate pre-set at 3 lpm.

Maximum hygiene: no manual contact with tap, reduced stagnation solenoid valve, duty flush prevents bacterial development. Supplied with fixings.

Weight: 4.1kg.

30-year warranty.