**Shower hose retaining collar**

For shower grab bars Ø 25-35mm

Reference: **830**

Specification description

Shower hose retaining collar for shower riser rails Ø 25 to 35mm and flexible hoses.

Install in addition to the shower head holder; fixes to the shower hose.

Retaining device: prevents shower head from coming into direct contact with the floor or the floor trap (source of bacterial contamination).

30-year warranty.