**KOMPACT washbasin and floor-standing WC combination**

Polished satin 304 stainless steel - Wall-mounted - floor WC left

With cistern

Reference: **162700**

Specification description

Washbasin combination unit with cistern, floor-standing WC pan on left side with recessed toilet roll holder.

Wall-mounted installation with 3 access panels, 2 on the sides and 1 on the top with theft prevention TORX security screws.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel body thickness: 2mm.

Rounded corners and edges for improved safety.

Smooth surface is easy to clean.

Suitable for prisons, police stations, etc.

WC pan is completely welded to washbasin, no screws: makes cleaning easier and prevents concealment of objects.

Washbasin equipped with time flow tap: stainless steel tamperproof push-button and anti-blocking system, 7 second time flow, M½".

WC fitted with 6-litre cistern.

Water inlets: washbasin M½", WC M3/8".

Recessed horizontal water outlet: Ø 100mm.

Supplied with washbasin siphon.

Easy to install: only one water outlet for both washbasin and WC,water inlet and outlet already connected.

Weight: 36kg.