**Twin hole pre-rinse mixer set with swivelling tubular spout**

With bib tap and swivelling tubular spout

Black flexible and scale-resistant handset

Reference: **5833**

Specification description

Complete pre-rinse set with bib tap suitable for intensive use in professional kitchens.

Deck-mounted twin hole mixer with 150mm centres with:

- valve heads with reinforced mechanisms and ergonomic controls.

- offset inlet connections with M1/2" tails.

Bib tap with swivelling tubular spout L. 200mm.

- 25 lpm full flow rate achieved within 1/4-turn.

- valve head with reinforced mechanism and ergonomic control.

Black handset with adjustable jet and 10 lpm flow rate at the outlet (ref. 433009).

Scale-resistant handset with shock-resistant tip.

Black, reinforced food-grade flexible hose L. 0.95m.

3/4" brass column.

Stainless steel spring guide.

30-year warranty.

These pre-rinse sets can be installed close to the splashback.