**BLACK BINOPTIC electronic tap**

Mains supply, H. 250mm

Spout with smooth interior

Reference: **398035**

Specification description

Deck-mounted electronic basin tap:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush 60 seconds every 24 hours after last use).

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Chrome-plated brass body.

Matte black chrome finish.

PEX flexible with filter and solenoid valve M⅜".

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Spout with smooth interior and low water volume (reduces bacterial development).

Drop height 250mm, for countertop washbasins.

Suitable for people with reduced mobility.

30-year warranty.