**TEMPOSTOP time flow shower kit**

Time flow, anti-blocking system (AB)

Cross wall 200 mm, AB, ROUND shower head

Reference: **747110**

Specification description

Time flow shower kit for cross wall installation:

TEMPOSTOP time flow valve M½" for mixed water supply.

For walls ≤ 200mm.

Time flow ~15 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated ROUND shower head, tamperproof and scale-resistant with automatic flow rate regulation.

Chrome-plated metal control.

Concealed fixing and anti-rotating pin.

Threaded rods can be cut to size.

AB anti-blocking system: water only flows when push-button is released.

30-year warranty.

[Formerly ref: 747214]