**TEMPOSTOP time flow urinal valve**

Time flow 3 seconds

Cross wall 200mm

Reference: **777110**

Specification description

Cross wall time flow urinal valve:

For standard or siphon action urinals.

For walls ≤ 200mm.

Compatible with rain water.

Time flow ~3 seconds.

Flow rate pre-set at 0.15 l/sec at 3 bar, can be adjusted.

Chrome-plated metal body M½".

Push-button base with anti-rotation nut.

Solid brass connection nut.

Cut-to-size threaded rod.

30-year warranty.

[Formerly ref: 777200]