**TEMPOFLUX 1 direct flush kit**

Time flow direct flush WC valve

Cross wall 200mm with tube

Reference: **761210**

Specification description

Flush system without cistern: directly connected to pipework.

For walls ≤ 200mm.

Soft-touch operation.

Time flow ~7 seconds.

Vacuum breaker.

Stopcock and flow rate/volume adjuster are integrated.

Chrome-plated metal body.

Inline inlet M¾".

Connection washer Ø 32/55mm.

Threaded rod can be cut to size.

Upstream supply pipes: minimum Ø 20mm required at all points (including connectors).

Base flow rate: 1 l/sec at 1 bar pressure.

With PVC flush tube Ø 32mm.

Compatible with rain water.

Suitable for people with reduced mobility.

30-year warranty.

[Formerly ref: 761700]