**Recessed waterproof housing for SECURITHERM shower**

Waterproof, kit 1/2

Recessed

Reference: **792BOX**

Specification description

Waterproof housing kit 1/2:

For thermostatic shower mixer.

Partition thickness can be between 16 to 30mm.

30-year warranty.

Order with control plate references: 792452, 792459, 792218 or 792219.