**TEMPOFLUX 3 control plate for WCs**

Time flow valve with soft-touch operation, AB, recessed

Dual flush plate 3L/6L - Black glass

Reference: **763030**

Specification description

Control plate and recessed TEMPOFLUX 3 time flow direct flush valve, kit 2/2:

Flush system without cistern: directly connected to pipework.

Black glass plate 205 x 190mm.

Mechanical fixing of the control plates.

TEMPOFLUX 3 F¾" valve compatible compatible with sea water, rain water and grey water.

Soft-touch operation.

AB anti-blocking system: only flows when push-button is released.

Dual flush 3L/6L can be adjusted to 2L/4L. Rectangular design.

Complies with European standard EN 12541 (acoustic level class II).

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Suitable for rimless WC pans without flow rate regulation and suitable for people with reduced mobility.

30-year warranty.

Order with frame system references 564065DE or 564060DE, or with 763BOX recessed housing.