**Electronic control unit**

For TEMPOMATIC 3 urinals

Battery-operated

Reference: **479446**

Specification description

Electronic control unit.

For TEMPOMATIC 3 urinals.

Power supplied by 6V batteries.

Dimensions: 57 x 40 x 23mm.