**BIOSAFE hygienic outlet M24/100**

1 peice

Reference: **922640**

Specification description

BIOSAFE hygienic free flow outlet M24/100 for product ranges 2564, 2565 and 2640.

No grid or partitions in contact with water.

Flow rate 5 lpm.

Water cannot stagnate in internal parts, reducing bacterial development.

Made from Hostaform®; reduces scale build-up.

Chrome-plated brass ring.

Supplied individually.

For installation only on a mixer or tap with a restricted flow rate to ensure a laminar flow with no splashing.