**Electronic control unit**

For TEMPOMATIC urinals and showers

Mains supply

Reference: **487449**

Specification description

Electronic control unit.

Electronic unit for TEMPOMATIC urinal and shower valve.

Works with a 12V mains supply.

Dimensions: 75 x 75 x 37mm.