**Detector**

For TEMPOMATIC

0.7m cable

Reference: **495070**

Specification description

Detector.

For TEMPOMATIC basin, shower, urinal and WC.

With 0.70m cable.