**TEMPOMATIC electronic basin tap valve**

Mains supply

For panels, without spout

Reference: **447100**

Specification description

Electronic basin tap valve for panel installation:

Mains supply with 3/8" solenoid valve.

230/12V transformer.

Independent IP65 electronic control unit.

Flow rate pre-set at 3 lpm at 3 bar.

Active, infrared presence detection.

Adjustable presence detection range.

Adjustable duty flush function (pre-set to ~60 seconds every 24h after last use).

Installation for panels from 1 - 12mm.

Anti-blocking feature.

Suitable for people with reduced mobility.

30-year warranty.