**Electronic control unit**

For TEMPOMATIC cross wall urinal

12V without transformer

Reference: **428112**

Specification description

Electronic control unit.

For individual urinals.

For TEMPOMATIC urinal valve, cross wall.

Works with a 12V power supply.

Transformer not included.

Dimensions: 105 x 105 x 60mm.