**Detector**

For BINOPTIC and TEMPOMATIC 2

With 0.70m cable

Reference: **CEL378V**

Specification description

Detector.

For BINOPTIC and TEMPOMATIC 2 basin controls.

With 0.70m cable.