**Hygiene washbasin with high upstand**

Polished satin 304 stainless steel

With two tap holes, Ø 22mm and Ø 30mm

Reference: **188300**

Specification description

Wall-hung healthcare washbasin with 450mm upstand.

Ideal for hospitals, healthcare establishments and medical practices.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 1.2mm.

With two tap holes, Ø 22mm and Ø 30mm, one above the other for electronic unit.

Smooth surface and rounded inside edges for easy cleaning.

Deep bowl reduces the risk of splashing ensuring a comfortable hand-washing experience.

Supplied with 1¼" waste. Without overflow.

CE marked. Complies with European standard EN 14688.

Weight: 10.2 kg.

30-year warranty.