**Time flow cartridge**

Mechanism for TEMPOFLUX WC

Time flow ~7 seconds

Reference: **743761**

Specification description

Time flow cartridge for TEMPOFLUX WC valve.

Push-button with soft-touch operation.

For exposed 3/4" WC flush valve.

Time flow ~7 seconds.

Base flow rate: 1lpm at 1 bar dynamic pressure.