**WC Cartridge**

For TEMPOFLUX

Time flow ~7 seconds

Reference: **743762**

Specification description

TEMPOFLUX WC cartridge:

Push-button with soft-touch operation.

For WC 3/4" recessed flush valve.

Timeflow ~7 seconds.

Base flow rate: 1L/sec at 1 bar dynamic pressure.