**Time flow cartridge**

Mechanism for TEMPLOFLUX 2 WC

Time flow ~7 seconds

Reference: **743622**

Specification description

Time flow cartridge for TEMPOFLUX 2 WC valve.

For recessed or with frame system WC valve.

Recessing depth: 10 to 35 mm.

Adjustable flow rate.

Time flow ~7 seconds.