**Time flow cartridge**

Mechanism for TEMPLOFLUX 2 WC

Time flow ~7 sec.s

Reference: **743677**

Specification description

Time flow cartridge for TEMPOFLUX 2 WC valves.

For recessed WC valves or frame-system mounted WC valves.

Flow rate can be adjusted.

Time flow ~7 seconds.