**Time flow cartridge**

Mechanism for TEMPLOFLUX 3 WC

Time flow ~7 seconds

Reference: **743765**

Specification description

Time flow cartridge for TEMPOFLUX 3 WC valves.

For recessed WC valves or frame-system mounted WC valves.

With anti-blocking mechanism.

Flow rate can be adjusted.

Time flow ~7 seconds.