**TEMPOMIX 3 AB time flow mixer**

Soft-touch operation, stopcocks Ø 15mm, AB system

Single control

Reference: **79400015AB**

Specification description

Deck-mounted single control time flow basin mixer:

Soft-touch operation.

Temperature control and operation on the push-button.

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated solid brass body.

PEX flexibles F3/8" with stopcocks, filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

Adjustable maximum temperature limiter.

AB anti-blocking security: water will flow only when the push-button is released.

Suitable for people with reduced mobility.

30-year warranty.