**BIOCLIP mechanical basin mixer**

Removable mechanical basin mixer H. 95mm L. 120mm, Hygiene lever

Stopcocks

Reference: **28216L**

Specification description

Deck-mounted mechanical basin mixer.

BIOCLIP mechanical mixer: mixer can be removed completely for cleaning and disinfection.

Single hole mixer with straight spout H. 95mm L. 120mm fitted with a hygienic flow straightener.

Ø 40mm ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interior and very low water volume.

Flow rate limited to 5 lpm at 3 bar.

Hygiene control lever L. 150mm.

With no pop-up waste.

Copper tails supplied with chrome-plated brass stopcocks.

Fixing reinforced by two stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.

Also available with PEX flexibles.