**TEMPOSOFT MIX 2 time flow mixer**

Soft-touch operation, Ø 15mm stopcocks

Standard temperature control lever, copper tails

Reference: **74250015CO**

Specification description

Deck-mounted time flow basin mixer:

Soft-touch operation.

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated solid brass body.

Copper tails with stopcocks, filters, non-return valves and Ø 15mm conical inlets.

Fixing reinforced by 2 stainless steel rods.

Side temperature control with standard lever and maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.