**TEMPOMATIC 4 electronic tap**

Integrated batteries, stopcock Ø 15mm

Integrated electronics, copper tails

Reference: **44000615CO**

Specification description

Deck-mounted electronic basin tap:

Battery-operated with integrated CR123 6V Lithium batteries.

Reduced stagnation solenoid valve and electronic unit integrated into the body of the tap.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after last use).

Presence detection sensor at the end of the spout optimises detection.

Chrome-plated stainless steel body.

Cap fixed in place by two concealed screws.

Copper tails with stopcock, filter and Ø 15mm conical inlet.

Fixing reinforced by two stainless steel rods.

Anti-blocking security.

Suitable for people with reduced mobility.

30-year warranty.