**BINOPTIC 2 electronic tap**

Mains, deck-mounted, stopcock, H. 170mm

Smooth interior spout, chrome-plated

Reference: **37401015**

Specification description

Deck-mounted satin electronic basin tap:

230/6V mains supply.

Reduced stagnation solenoid valve and electronic unit integrated into the body of the tap.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant aerator.

Adjustable duty flush (~60 seconds every 24 hours after the last use).

Stainless steel tap, 170mm high for semi-recessed basins.

Presence detection sensor at the end of the spout optimises detection.

PEX flexibles Ø 15mm for compression fittings with filters and stopcock.

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Smooth spout interior with low water volume (reduces bacterial development).

Set detection distance, duty flush and launch thermal shocks manually.

Suitable for people with reduced mobility.

30-year warranty.