**Be-Line® comfort backrest for WCs**

Matte black powder-coated aluminium structure

Black polyurethane

Reference: **511928BK**

Specification description

Be-Line® comfort backrest for WCs for people with reduced mobility.

Matte black powder-coated aluminium structure.

Flexible polyurethane backrest for toilets.

Dimensions: 150 x 513 x 173mm.

30-year warranty.

CE marked.