**Time flow cartridge**

For TEMPOSTOP and TEMPOMIX 2 cross wall/lever basin

Time flow ~7 seconds, AB anti-blocking system

Reference: **743205**

Specification description

Time flow cartridge for TEMPOSTOP and TEMPOMIX 2 cross wall/lever basin.

Time flow ~7 seconds.