**TEMPOMATIC 4 electronic soap dispenser**

Liquid soap, foam soap or hydroalcoholic gel dispenser

Mains, chromed 304 stainless steel, cross wall

Reference: **512171P**

Specification description

Wall-mounted electronic soap dispenser.

Liquid soap, foam soap or hydroalcoholic gel dispenser.

Vandal-resistant model for cross wall up to 110mm.

No manual contact: infrared cell detects hands automatically.

Chrome-plated 304 stainless steel spout.

No waste dose dispenser.

Separate electronic unit and removable tank for installation beneath the washbasin or in a service duct.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with maximum viscosity of 3,000 mPa.s or specific foam soap.

Total spout length: 135mm.

Supplied with flexible tube 1.20m for remote tanks (tank not supplied).

30-year warranty.

CE marked.