**Solenoid valve**

For washbasin controls TEMPOMATIC 3 and TEMPOMATIC MIX 3

With flow rate adjustor - M28 - 6 V

Reference: **479651**

Specification description

Piston operated solenoid valve with flow rate adjustor.

For TEMPOMATIC 3 washbasin controls.

For TEMPOMATIC MIX 3 washbasin controls (before May 2023).

Works with a 6V power supply.

Dimensions: 35 x 38mm, M28 x 1,0.