**TEMPOMATIC 4 recessed housing for showers**

Batteries, kit 1/2

Recessed, waterproof

Reference: **443PBOX**

Specification description

Waterproof recessed housing for TEMPOMATIC 4 for showers, kit 1/2:

Collar with waterproof seal.

Hydraulic connection from the outside and maintenance from the front.

Adjusts to all types of installations (rails, solid walls, panels).

Compatible with wall finishes 10 - 120mm (while maintaining the minimum recessing depth of 93mm).

Stopcocks and flow rate adjustment, filters, non-return valves and cartridge are all integrated and accessible from the front.

Supplied in 2 kits: secure system flush without sensitive elements.

30-year warranty.

Order with control plate reference 443218.