**Recessed nanny joint for SPORTING 2 SECURITHERM**

For SPORTING 2 SECURITHERM battery-operated or time flow - Kit 1/2

Compact, top or bottom inlet

Reference: **714612**

Specification description

Recessed nanny joint, kit 1/2:

Compact nanny bracket for SPORTING 2 SECURITHERM battery-operated or time flow shower panels.

Recessed top or bottom inlet.

Delivered with buttons pre-mounted for pressure test.

Fixing plate is easy to install: bayonette system to allow maintenance of the caps in situ.

Mounted with screwdriver or pliers.

Modular installation (plaster rails, solid walls):

- Installation with plaster rails (with or without struts): compatible with panels between 24 and 68mm (with a minimum recessing depth of 48mm).

- Installation with solid walls: compatible with panels between 0 and 68mm.

Secured system purge without sensitive elements.

Connector M1/2".

30 year warranty.

Order with the SPORTING 2 SECURITHERM battery-operated shower panel with recessed supply, reference 714916, or the time flow SPORTING 2 SECURITHERM shower panel with recessed supply, references 714735 or 714735AB.