**TEMPOSTOP MIX 4 time flow basin mixer**

Without stopcocks

Side temperature control lever

Reference: **704910**

Specification description

Deck-mounted time flow basin mixer:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated solid brass body

F3/8" PEX flexibles with filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

Side temperature control with standard lever and adjustable maximum temperature limiter.

30-year warranty.