**TEMPOMATIC MIX 5 electronic basin mixer**

Mains supply, recessed, wall-mounted

For panels, L. 180mm, integrated electronics

Reference: **499410**

Specification description

Cross-wall electronic basin mixer:

Mains supply 230/6V.

Electronics and reduced stagnation solenoid valve integrated into the body of the mixer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after last use).

Presence detection sensor at the end of the spout optimises detection.

Chrome-plated metal body.

Anti-blocking feature prevents misuse.

Temperature control with adjustable temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.