**Nanny joint for recessed water inlets**

For battery-operated mixers, Kit 1/2

Reference: **484612**

Specification description

Nanny joint for recessed water inlet, Kit 1/2 :

For wall-mounted TEMPOMATIC MIX 4, connects directly to the pipework.

Compatible with mixers operated by CR123 6V lithium batteries.

Adaptable installation (plaster rails, solid walls, panels).

Compatible with wall finishes from 0 to 35mm.

Secured system purge without sensitive elements.

30-year warranty.

Order with basin mixer references 493506 or 493406.