**Basic straight grab bar, white, Ø 32mm, 300mm**

White powder-coated stainless steel

Ø 32mm

Reference: **35050W**

Specification description

Basic straight grab bar for people with reduced mobility.

Ø 32mm tube, 300mm centres.

Grab bar made from white powder-coated stainless steel.

Concealed fixings, secured to wall by a 3-hole stainless steel plate.

30-year warranty.

CE marked.