**Cover plate for drop-down grab bar**

Bright white anti-bacterial HR Nylon

Reference: **510150N**

Specification description

Birght white HR Nylon cover plate for drop-down rails.

NylonClean anti-bacterial treatment: optimal protection against bacterial development.

Hides the fixing screws when the drop-down rail is removed.

Reduces the number of drop-down rails required in a building, allowing installation only when required. For example: hotels or hospitals temporarily accommodating a person with reduced mobility.

Supplied with stainless steel screws for concrete walls.

30-year warranty.