**Towel rail**

Ø 20mm, 1 rail

Bright polished stainless steel

Reference: **510788P**

Specification description

Single towel rail for bathrooms.

Designer towel rail.

Robust model.

Ø 20mm rail, length 600mm.

Bright polished bacteriostatic 304 stainless steel.

Wall-mounted towel rail with concealed fixings.

30-year warranty.