**Straight curtain rail**

Cut-to-size

Length 2m

Reference: **356**

Specification description

Cut-to-size straight curtain rail.

Rod for shower curtains made from bright polished 304 stainless steel tube, 1mm thick.

Dimensions: Ø 16mm - 2m.

30-year warranty.