**Angled curtain rail**

Fixed

0.80 x 0.80m

Reference: **361**

Specification description

Fixed, angled shower curtain.

Rod for angled shower curtain made from bright polished 304 stainless steel, 1mm thick

Dimensions: Ø 16mm - 0.80 x 0.80m.

30-year warranty.