**Complete bed pan cleaner**

With stopcock M1/2"

HOSPITAL bed pan cleaner with inverted hand spray

Reference: **2592**

Specification description

Complete bed pan cleaner with stopcock with ceramic discs.

Integrated back flow prevention device and non-return valve.

White, opaque reinforced PVC flexible hose, FF1/2" L. 0.80m.

HOSPITAL bed pan cleaner with inverted hand spray: water flows when trigger is released (shut off the stopcock after use to avoid the flexible remaining under constant pressure) with removable nozzle at a 30° angle.

White, wall-mounted hook with screw.

30-year warranty.