**Pre-rinse set with mixer**

With bib tap and swivelling telescopic spout

White scale-resistant hand spray

Reference: **G6632**

Specification description

Complete pre-rinse set with bib tap.

Suitable for intensive use in professional kitchens.

Single hole deck-mounted mixer with:

- valve head with control knobs.

- F3/8" flexible connectors and non-return valves.

- reinforced fixing via 2 threaded rods and back-nuts.

Bib tap with:

- telescopic, swivelling spout L. 200 - 290mm with 20 lpm flow rate at the outlet.

- valve head with control knob.

White hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433000).

Scale-resistant hand spray and shock-resistant tip.

White, reinforced, food-grade flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.