**TEMPOSTOP time flow tap**

Wall-mounted, ½" with wall plate

Reference: **746292**

Specification description

Wall-mounted time flow basin tap:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 15 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated brass body with wall plate M½".

30-year warranty.