**Pre-mixer Compact**

For basins ½"

Reference: **200000**

Specification description

For installation beneath single basin.

Nickel-plated body MF½".

Non-return valves and filters can be checked.

30-year warranty.